Write an assembly language program to swap two 8-bit data using 8085 processor

PROGRAM:

LDA 2500

MOV B,A

LDA 2501

STA 2503

MOV A,B

STA 2504

HLT

OUTPUT:

